SECTION 08 43 12

Ballistic Resistant SafeShutter™

*Copyright 2020 - 2020 SafeWood Designs, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* SafeWood Designs, Inc.; ballistic resistant wood framed storefront, doors, and windows.  
This section is based on the products of SafeWood Designs, Inc., which is located at:  
7281 Commerce Cir. W.  
Fridley, MN 55432  
Tel: 844-896-1800  
Email:[request info (sales@safewooddesigns.com)](http://admin.arcat.com/users.pl?action=UserEmail&company=SafeWood+Designs,+Inc.&coid=52745&rep=&fax=&message=RE:%20Spec%20Question%20(08411wdd):%20%20&mf=)  
Web:<http://safewooddesigns.com>  
[[Click Here](http://www.arcat.com/arcatcos/cos52/arc52745.html)] for additional information.  
We established SafeWood Designs because our changing world means that safety and security needs are increasing and gun violence is a very real threat. An unfortunate threat to our schools, homes, places of worship, offices, and businesses.  
In today's market nearly all ballistic doors, walls and room products are "cookie cutter", often leaving your home or business looking and feeling like a prison.  
Why should having safety and security mean losing warmth and elegance? In an ideal world, all secure surroundings would be beautiful, blending with existing millwork and furnishings completely undetected.  
At SafeWood Designs you can have both beauty and safety.

1. GENERAL
   1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. Ballistic resistant features
       1. SafeShutter™
  1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 06 40 00 - Architectural Woodwork.
    2. Section 09 21 16 Gypsum Wall Assemblies
  1. REFERENCES

\*\* NOTE TO SPECIFIER \*\* Delete references from the list below that are not actually required by the text of the edited section.

* + 1. ASTM International (ASTM):
       1. ASTM C1036 - Standard Specification for Flat Glass.
       2. ASTM C1048 - Standard Specification for Heat-Strengthened and Fully Tempered Flat Glass.
       3. ASTM C1349 - Standard Specification for Architectural Flat Glass Clad Polycarbonate.
       4. ASTM D523 - Standard Test Method for Specular Gloss.
       5. ASTM E90 - Standard Method for Laboratory Measurement of Airborne Sound Transmission Loss of Building Partitions.
       6. ASTM E119 - Standard Test for One-Hour Fire-Rating of Building Construction and Materials.
       7. ASTM E413 - Classification for Sound Insulation Rating.
       8. ASTM E1332 - Classification for Determination of Outdoor-Indoor Transmission Class.
       9. ASTM F1233 - Standard Test Method for Forced Entry Testing of Materials and Assemblies.
    2. American National Standards Institute (ANSI):
       1. ANSI Z97.1 - For Safety Glazing Materials Used In Buildings - Safety Performance Specifications And Methods Of Test.
    3. Architectural Woodwork Institute (AWI):
       1. AWI Architectural Woodwork Standards.
    4. Consumer Product Safety Commission (CPSC):
       1. CPSC 16 CFR 1201 - Safety Standard for Architectural Glazing Materials.
    5. International Organization for Standardization:
       1. ISO 9001 - Quality Management System.
    6. National Hardwood Lumber Association (NHLA).
    7. National Institute of Justice (NIJ):
       1. NIJ Standard 0108.01 - Ballistic Standards.
    8. U.S. Department of State:
       1. The International Traffic in Arms Regulations (ITAR).
    9. Underwriters Laboratories (UL):
       1. UL 752 - Specifications and Ammunition, Standard for Bullet Resisting Equipment.
  1. SUBMITTALS
     1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
     2. Product Data:
        1. Manufacturer's data sheets on each product to be used.
        2. Preparation instructions and recommendations.
        3. Storage and handling requirements and recommendations.
        4. Typical installation methods.

\*\* NOTE TO SPECIFIER \*\* Delete if not applicable to product type.

* + 1. Shop Drawings: Include details of materials, construction and finish. Include relationship with adjacent construction.
  1. QUALITY ASSURANCE
     1. Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with substantial similar project experience.
     2. Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
     3. Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.

\*\* NOTE TO SPECIFIER \*\* Include mock-up if the project size or quality warrant the expense. The following is one example of how a mock-up on might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project.

* 1. DELIVERY, STORAGE, AND HANDLING
     1. Store and handle in strict compliance with manufacturer's written instructions and recommendations.
     2. Protect from damage due to weather, excessive temperature, and construction operations.
  2. PROJECT CONDITIONS
     1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not store or install products under environmental conditions outside manufacturer's recommended limits.
     2. Maintain temperature and humidity in installation area as required to maintain moisture content of installed woodwork within acceptable limits as defined by AWI, from at least two days prior to the date of product arrival through the remainder of construction period.
     3. Do not deliver or install woodwork until building is enclosed, wet work is complete, and HVAC system is operating and maintaining temperature between 60 and 90 degrees F (16 and 32 degrees C) and relative humidity as directed by AWI for the appropriate region during the remainder of the construction period and the warranty period.
  3. WARRANTY
     1. Manufacturer's Warranty: Provide manufacturer's standard limited warranty.

1. PRODUCTS
   1. Product: SafeWood Designs SafeShutter™ Model Number:
      1. SafeShutter™ Opening up to 36” x 72” Model Number: SS-WB-3060-WHWHI-UL03
      2. SafeShutter™ Opening up to 36” x 84” Model Number: SS-WB-3070-WHWHI-UL03
      3. SafeShutter™ Opening up to 42” x 72” Model Number: SS-WB-3660-WHWHI-UL03
      4. SafeShutter™ Opening up to 42” x 84” Model Number: SS-WB-3670-WHWHI-UL03

**\*\*\*NOTE TO SPECIFIER \*\* Change PAMAL to the desired finish and change the last two numbers to the required UL Level to adjust the part number. \*\*\* Please call for any clarifications.**

* 1. MANUFACTURERS
     1. Acceptable Manufacturer: SafeWood Designs, Inc., which is located at: 7281 Commerce Cir. W.; Fridley, MN 55432; Tel: 844-896-1800; Email: [request info (sales@safewooddesigns.com)](mailto:request%20info%20(sales@safewooddesigns.com)); Web <http://www.safewooddesigns.com>

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
  1. PERFORMANCE REQUIREMENTS
     1. Standards Compliance:
        1. Perform work in accordance with Quality Standards of the Architectural Woodwork Institute to a Custom quality.
        2. Manufactured in the USA.
     2. Ballistic Resistance:
        1. Bullet resistance of joints equal to that of the panel.
        2. Non-ricochet type doors and frames to permit the capture and retention of an attacking projectile lessening the potential of a random injury or lateral penetration.
        3. Window, frame, and door components shall effectively reduce the penetration potential of bullets at all seams and gaps between different wall construction components.
        4. Ballistic Rating, UL 752: Level 3.
  2. BALLISTIC RESISTANT WOOD STOREFRONTS

\*\* NOTE TO SPECIFIER \*\* Modify configuration paragraph as required to meet project requirements.

* + 1. Configuration: As indicated on Drawings.
    2. Materials:

\*\* NOTE TO SPECIFIER \*\* Delete materials not required.

* + - 1. Fiberglass: Pultruded ballistic grade fiberglass impregnated with thermoset resin constructed into rigid flat sheets.
         1. Fire Rating, ASTM E119: 1 hour.
         2. Self-Extinguishing UL 94-V-0

\*\* NOTE TO SPECIFIER \*\* Delete thickness options not required.

* + - * 1. Thickness, UL Level 3: 1/2 inch (12 mm).
      1. Plastic Laminate:

\*\* NOTE TO SPECIFIER \*\* Delete plastic laminate style options not required.

* + - * 1. Style: As indicated on Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete door options not required.

* + 1. Fabrication:
       1. Wood Moisture Content: Comply with requirements of referenced quality standard for wood moisture content in relation to ambient relative humidity during fabrication and in installation areas.
       2. Complete fabrication, including assembly, finishing, and hardware application, to maximum extent possible before shipment to Project site. Disassemble components only as necessary for shipment and installation.
          1. Where necessary for fitting at site, provide ample allowance for scribing, trimming, and fitting.
          2. Trial fit assemblies at fabrication shop that cannot be shipped completely assembled.
          3. Install dowels, screws, bolted connectors, and other fastening devices that can be removed after trial fitting.
          4. Verify that various parts fit as intended and check measurements of assemblies against field measurements indicated on Shop Drawings before disassembling for shipment.
    2. Finishes:
       1. General: To the greatest maximum possible, finish Ballistic Resistant Features at fabrication shop as specified in this Section. Defer only final touchup, cleaning, and polishing until after installation.

1. EXECUTION
   1. EXAMINATION
      1. Do not begin installation until substrates have been properly constructed and prepared.
      2. If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
   2. PREPARATION
      1. Clean surfaces thoroughly prior to installation.
      2. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
   3. INSTALLATION
      1. Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
      2. Adjust doors and hardware for proper operation.
   4. CLEANING AND PROTECTION
      1. Clean products in accordance with the manufacturer's recommendations.
      2. Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION